Fastening the "Easyfit" Bell Muffle to the Clapper
(manufacturers original instructions)
NOTE: 
Do not attempt to fit or remove the muffle when the bell is raised. 
This is neither practical or safe.

(1) 
The ends of the straps are held using the specially designed stainless steel split rings supplied. Before presenting the muffle to the clapper, place one ring through the left hand loop of the top strap, and one through the right hand loop of the bottom strap. In each case, the straight section of the ring should point away from the pad part of the muffle. 
See diagram (1)

(2) 
Working on the opposite side of the clapper to the muffle, first fasten the top strap as follows. Pull both ends of the strap round the clapper shaft to your side. Bring the free end of the strap through the ring from the back. 
See diagram (2) 

Pull the strap tight, then take the free end of the strap back round the far side of the clapper to the open end of the ring. Twist the ring anticlockwise (using the straight section)to facilitate threading the open end through the loop in the strap. Twist back to the vertical position to secure. 
See diagrams (3) & (4).

(3) 
Attach the bottom strap using the same principle as for the top strap.

(4) 
To remove the muffle, simply twist the rings to release the straps.
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